CLEAN THE PCB OR COPPER CLAD

APPLY PHOTO RESISTOR AND UV DEVLOPER



DRY THE BOARD 4MIN

EXPOSE TO UVLIGHT FOR 2MIN





DEVELOP THE IMAGE







ETCH THE COPPER CLAD





DRILLING



SOLDERING